Main Page Modules Alphabetical List Data Structures File List Data Fields Globals # Defines for IOCTL Commands [IXP425 UART Access (IxUARTAcc) API] IOCTL Commands (Request codes) which can be used with ixUARTIoctl. More...
## Defines
#define | IX_BAUD_SET
| Set the baud rate.
#define | IX_BAUD_GET
| Get the baud rate.
#define | IX_MODE_SET
| Set the UART mode of operation.
#define | IX_MODE_GET
| Get the current UART mode of operation.
#define | IX_OPTS_SET
| Set the UART device options.
#define | IX_OPTS_GET
| Get the UART device options.
#define | IX_STATS_GET
| Get the UART statistics.
## Detailed Description IOCTL Commands (Request codes) which can be used with ixUARTIoctl. ## Define Documentation
#define IX_BAUD_GET
| Get the baud rate. Definition at line 165 of file IxUART.h.
#define IX_BAUD_SET
| Set the baud rate. Definition at line 156 of file IxUART.h.
#define IX_MODE_GET
| Get the current UART mode of operation. Definition at line 181 of file IxUART.h.
#define IX_MODE_SET
| Set the UART mode of operation. Definition at line 172 of file IxUART.h.
#define IX_OPTS_GET
| Get the UART device options. Definition at line 199 of file IxUART.h.
#define IX_OPTS_SET
| Set the UART device options. Definition at line 190 of file IxUART.h.
#define IX_STATS_GET
| Get the UART statistics. Definition at line 208 of file IxUART.h.
Automatically generated from sources. © Intel Corp. 2003