Main Page Modules Alphabetical List Data Structures File List Data Fields Globals # Defines for Default Values [IXP425 UART Access (IxUARTAcc) API] Default values which can be used for UART configuration. More...
## Defines
#define | IX_UART_DEF_OPTS
| The default hardware options to set the UART to - no flow control, 8 bit word, 1 stop bit, no parity.
#define | IX_UART_DEF_XMIT
| The default UART FIFO size - must be no bigger than 64.
#define | IX_UART_DEF_BAUD
| The default UART baud rate - 9600.
#define | IX_UART_MIN_BAUD
| The minimum UART baud rate - 9600.
#define | IX_UART_MAX_BAUD
| The maximum UART baud rate - 926100.
#define | IX_UART_XTAL
| The UART clock speed.
## Detailed Description Default values which can be used for UART configuration. See also: ixUARTDev ## Define Documentation
#define IX_UART_DEF_BAUD
| The default UART baud rate - 9600. Definition at line 108 of file IxUART.h.
#define IX_UART_DEF_OPTS
| The default hardware options to set the UART to - no flow control, 8 bit word, 1 stop bit, no parity. Definition at line 90 of file IxUART.h.
#define IX_UART_DEF_XMIT
| The default UART FIFO size - must be no bigger than 64. Definition at line 99 of file IxUART.h.
#define IX_UART_MAX_BAUD
| The maximum UART baud rate - 926100. Definition at line 126 of file IxUART.h.
#define IX_UART_MIN_BAUD
| The minimum UART baud rate - 9600. Definition at line 117 of file IxUART.h.
#define IX_UART_XTAL
| The UART clock speed. Definition at line 135 of file IxUART.h.
Automatically generated from sources. © Intel Corp. 2003