Main Page Modules Alphabetical List Data Structures File List Data Fields Globals # ixUARTDev Struct Reference [IXP425 UART Access (IxUARTAcc) API, IXP425 UART Access (IxUARTAcc) API] Device descriptor for the UART. More...
## Data Fields
UINT8 * | addr
| device base address
ixUARTMode | mode
| interrupt, polled or loopback
int | baudRate
| baud rate
int | freq
| UART clock frequency.
int | options
| hardware options
int | fifoSize
| FIFO xmit size.
ixUARTStats | stats
| device statistics
## Detailed Description Device descriptor for the UART. Definition at line 342 of file IxUART.h. ## Field Documentation
UINT8* ixUARTDev::addr
| device base address Definition at line 344 of file IxUART.h.
int ixUARTDev::baudRate
| baud rate Definition at line 346 of file IxUART.h.
int ixUARTDev::fifoSize
| FIFO xmit size. Definition at line 349 of file IxUART.h.
int ixUARTDev::freq
| UART clock frequency. Definition at line 347 of file IxUART.h.
ixUARTMode ixUARTDev::mode
| interrupt, polled or loopback Definition at line 345 of file IxUART.h.
int ixUARTDev::options
| hardware options Definition at line 348 of file IxUART.h.
ixUARTStats ixUARTDev::stats
| device statistics Definition at line 351 of file IxUART.h.
The documentation for this struct was generated from the following file: IxUART.h
Automatically generated from sources. © Intel Corp. 2003