Main Page Modules Alphabetical List Data Structures File List Data Fields Globals # IxAtmmPortCfg Struct Reference [IXP425 ATM Manager (IxAtmm) API] Structure contains port-specific information required to initialize IxAtmm, and specifically, the IXP425 UTOPIA Level-2 device. More...
## Data Fields
unsigned | reserved_1:11
| [31:21] Should be zero
unsigned | UtopiaTxPhyAddr:5
| [20:16] Address of the transmit (Tx) PHY for this port on the 5-bit UTOPIA Level-2 address bus
unsigned | reserved_2:11
| [15:5] Should be zero
unsigned | UtopiaRxPhyAddr:5
| [4:0] Address of the receive (Rx) PHY for this port on the 5-bit UTOPIA Level-2 address bus
## Detailed Description Structure contains port-specific information required to initialize IxAtmm, and specifically, the IXP425 UTOPIA Level-2 device. Definition at line 191 of file IxAtmm.h. ## Field Documentation
unsigned IxAtmmPortCfg::reserved_1
| [31:21] Should be zero Definition at line 192 of file IxAtmm.h.
unsigned IxAtmmPortCfg::reserved_2
| [15:5] Should be zero Definition at line 197 of file IxAtmm.h.
unsigned IxAtmmPortCfg::UtopiaRxPhyAddr
| [4:0] Address of the receive (Rx) PHY for this port on the 5-bit UTOPIA Level-2 address bus Definition at line 198 of file IxAtmm.h.
unsigned IxAtmmPortCfg::UtopiaTxPhyAddr
| [20:16] Address of the transmit (Tx) PHY for this port on the 5-bit UTOPIA Level-2 address bus Definition at line 193 of file IxAtmm.h.
The documentation for this struct was generated from the following file: IxAtmm.h
Automatically generated from sources. © Intel Corp. 2003