Main Page Modules Alphabetical List Data Structures File List Data Fields Globals # Defines for IOCTL Arguments [IXP425 UART Access (IxUARTAcc) API] POSIX style IOCTL arguments which can be used with ixUARTIoctl. More...
## Defines
#define | CLOCAL
| Software flow control.
#define | CREAD
| Enable interrupt receiver.
#define | CSIZE
| Characters size.
#define | CS5
| 5 bits
#define | CS6
| 6 bits
#define | CS7
| 7 bits
#define | CS8
| 8 bits
#define | STOPB
| Send two stop bits (else one).
#define | PARENB
| Parity detection enabled (else disabled).
#define | PARODD
| Odd parity (else even).
## Detailed Description POSIX style IOCTL arguments which can be used with ixUARTIoctl. See also: ixUARTMode ## Define Documentation
#define CLOCAL
| Software flow control. Definition at line 230 of file IxUART.h.
#define CREAD
| Enable interrupt receiver. Definition at line 239 of file IxUART.h.
#define CS5
| 5 bits Definition at line 257 of file IxUART.h.
#define CS6
| 6 bits Definition at line 266 of file IxUART.h.
#define CS7
| 7 bits Definition at line 275 of file IxUART.h.
#define CS8
| 8 bits Definition at line 284 of file IxUART.h.
#define CSIZE
| Characters size. Definition at line 248 of file IxUART.h.
#define PARENB
| Parity detection enabled (else disabled). Definition at line 302 of file IxUART.h.
#define PARODD
| Odd parity (else even). Definition at line 311 of file IxUART.h.
#define STOPB
| Send two stop bits (else one). Definition at line 293 of file IxUART.h.
Automatically generated from sources. © Intel Corp. 2003