Main Page Modules Alphabetical List Data Structures File List Data Fields Globals # IxAtmdAccUtopiaConfig::UtTxDefineIdle_ Struct Reference [IXP425 ATM Driver Access (IxAtmdAcc) Utopia Control API] Utopia Tx idle cells Register. More...
## Data Fields
unsigned int | vpi:12
| [31:20] ATM VPI [11:0] OR GFC [3:0] and VPI [7:0] Note: if VCIdleTxGFC is set to 0 the GFC field is ignored in test
unsigned int | vci:16
| [19:4] ATM VCI [15:0]
unsigned int | pti:3
| [3:1] ATM PTI PTI [2:0] Note: if VCIdleTxPTI is set to 0 the PTI field is ignored in test.
unsigned int | clp:1
| [0] ATM CLP [0] Note: if VCIdleTxCLP is set to 0 the CLP field is ignored in test.
## Detailed Description Utopia Tx idle cells Register. Definition at line 1034 of file IxAtmdAccCtrl.h. ## Field Documentation
unsigned int IxAtmdAccUtopiaConfig::UtTxDefineIdle_::clp
| [0] ATM CLP [0] Note: if VCIdleTxCLP is set to 0 the CLP field is ignored in test. Definition at line 1045 of file IxAtmdAccCtrl.h.
unsigned int IxAtmdAccUtopiaConfig::UtTxDefineIdle_::pti
| [3:1] ATM PTI PTI [2:0] Note: if VCIdleTxPTI is set to 0 the PTI field is ignored in test. Definition at line 1042 of file IxAtmdAccCtrl.h.
unsigned int IxAtmdAccUtopiaConfig::UtTxDefineIdle_::vci
| [19:4] ATM VCI [15:0] Definition at line 1040 of file IxAtmdAccCtrl.h.
unsigned int IxAtmdAccUtopiaConfig::UtTxDefineIdle_::vpi
| [31:20] ATM VPI [11:0] OR GFC [3:0] and VPI [7:0] Note: if VCIdleTxGFC is set to 0 the GFC field is ignored in test Definition at line 1037 of file IxAtmdAccCtrl.h.
The documentation for this struct was generated from the following file: IxAtmdAccCtrl.h
Automatically generated from sources. © Intel Corp. 2003