Main Page Modules Alphabetical List Data Structures File List Data Fields Globals # IxHssAccHdlcMode Struct Reference [IXP425 HSS Access (IxHssAcc) API] This structure contains 56Kbps, HDLC-mode configuration parameters. More...
## Data Fields
BOOL | hdlc56kMode
| 56kbps(TRUE)/64kbps(FALSE) HDLC
IxHssAcc56kEndianness | hdlc56kEndian
| 56kbps data endianness ignored if hdlc56kMode is FALSE
BOOL | hdlc56kUnusedBitPolarity0
| The polarity '0'(TRUE)/'1'(FALSE) of the unused bit while in 56kbps mode ignored if hdlc56kMode is FALSE.
## Detailed Description This structure contains 56Kbps, HDLC-mode configuration parameters. Definition at line 590 of file IxHssAcc.h. ## Field Documentation
IxHssAcc56kEndianness IxHssAccHdlcMode::hdlc56kEndian
| 56kbps data endianness ignored if hdlc56kMode is FALSE Definition at line 593 of file IxHssAcc.h.
BOOL IxHssAccHdlcMode::hdlc56kMode
| 56kbps(TRUE)/64kbps(FALSE) HDLC Definition at line 592 of file IxHssAcc.h.
BOOL IxHssAccHdlcMode::hdlc56kUnusedBitPolarity0
| The polarity '0'(TRUE)/'1'(FALSE) of the unused bit while in 56kbps mode ignored if hdlc56kMode is FALSE. Definition at line 595 of file IxHssAcc.h.
The documentation for this struct was generated from the following file: IxHssAcc.h
Automatically generated from sources. © Intel Corp. 2003