Main Page Modules Alphabetical List Data Structures File List Data Fields Globals # USBDevice Struct Reference [IXP425 USB Driver Public API] USBDevice. More...
## Data Fields
UINT32 | baseIOAddress
| base I/O device address
UINT32 | interruptLevel
| device IRQ
UINT32 | lastError
| detailed error of last function call
UINT32 | deviceIndex
| USB device index.
UINT32 | flags
| initialization flags
UINT8 | deviceContext [USB_CONTEXT_SIZE]
| used by the driver to identify the device
## Detailed Description USBDevice. Definition at line 74 of file usbtypes.h. ## Field Documentation
UINT32 USBDevice::baseIOAddress
| base I/O device address Definition at line 76 of file usbtypes.h.
UINT8 USBDevice::deviceContext[USB_CONTEXT_SIZE]
| used by the driver to identify the device Definition at line 81 of file usbtypes.h.
UINT32 USBDevice::deviceIndex
| USB device index. Definition at line 79 of file usbtypes.h.
UINT32 USBDevice::flags
| initialization flags Definition at line 80 of file usbtypes.h.
UINT32 USBDevice::interruptLevel
| device IRQ Definition at line 77 of file usbtypes.h.
UINT32 USBDevice::lastError
| detailed error of last function call Definition at line 78 of file usbtypes.h.
The documentation for this struct was generated from the following file: usbtypes.h
Automatically generated from sources. © Intel Corp. 2003