Main Page Modules Alphabetical List Data Structures File List Data Fields Globals # IxAtmdAccUtopiaConfig::UtRxStatsConfig_ Struct Reference [IXP425 ATM Driver Access (IxAtmdAcc) Utopia Control API] Utopia Rx stats config Register. More...
## Data Fields
unsigned int | vpi:12
| [31:20] ATM VPI VPI [11:0] OR GFC [3:0] and VPI [7:0] Note: if VCStatsRxGFC is set to 0 the GFC field is ignored in test
unsigned int | vci:16
| [19:4] VCI [15:0] or PHY Address [4]
unsigned int | pti:3
| [3:1] PTI [2:0] or or PHY Address [3:1] Note: if VCStatsRxPTI is set to 0 the PTI field is ignored in test
unsigned int | clp:1
| [0] CLP [0] or PHY Address [0] Note: if VCStatsRxCLP is set to 0 the CLP field is ignored in test
## Detailed Description Utopia Rx stats config Register. Definition at line 1352 of file IxAtmdAccCtrl.h. ## Field Documentation
unsigned int IxAtmdAccUtopiaConfig::UtRxStatsConfig_::clp
| [0] CLP [0] or PHY Address [0] Note: if VCStatsRxCLP is set to 0 the CLP field is ignored in test Note: if VCStatsRxEnb is set to 0 only the PHY port address is used for statistics gathering.. Definition at line 1365 of file IxAtmdAccCtrl.h.
unsigned int IxAtmdAccUtopiaConfig::UtRxStatsConfig_::pti
| [3:1] PTI [2:0] or or PHY Address [3:1] Note: if VCStatsRxPTI is set to 0 the PTI field is ignored in test Note: if VCStatsRxEnb is set to 0 only the PHY port address is used for statistics gathering.. Definition at line 1360 of file IxAtmdAccCtrl.h.
unsigned int IxAtmdAccUtopiaConfig::UtRxStatsConfig_::vci
| [19:4] VCI [15:0] or PHY Address [4] Definition at line 1358 of file IxAtmdAccCtrl.h.
unsigned int IxAtmdAccUtopiaConfig::UtRxStatsConfig_::vpi
| [31:20] ATM VPI VPI [11:0] OR GFC [3:0] and VPI [7:0] Note: if VCStatsRxGFC is set to 0 the GFC field is ignored in test Definition at line 1355 of file IxAtmdAccCtrl.h.
The documentation for this struct was generated from the following file: IxAtmdAccCtrl.h
Automatically generated from sources. © Intel Corp. 2003