Main Page Modules Alphabetical List Data Structures File List Data Fields Globals # IxPerfProfAccBusPmuResults Struct Reference [IXP425 Performance Profiling (IxPerfProfAcc) API] Results obtained from running the Bus Pmu component. The results are obtained when the get functions is called. More...
## Data Fields
UINT32 | statsToGetLower27Bit [IX_PERFPROF_ACC_BUS_PMU_MAX_PECS]
| Lower 27 Bit of counter value.
UINT32 | statsToGetUpper32Bit [IX_PERFPROF_ACC_BUS_PMU_MAX_PECS]
| Upper 32 Bit of counter value.
## Detailed Description Results obtained from running the Bus Pmu component. The results are obtained when the get functions is called. Definition at line 189 of file IxPerfProfAcc.h. ## Field Documentation
UINT32 IxPerfProfAccBusPmuResults::statsToGetLower27Bit[IX_PERFPROF_ACC_BUS_PMU_MAX_PECS]
| Lower 27 Bit of counter value. Definition at line 191 of file IxPerfProfAcc.h.
UINT32 IxPerfProfAccBusPmuResults::statsToGetUpper32Bit[IX_PERFPROF_ACC_BUS_PMU_MAX_PECS]
| Upper 32 Bit of counter value. Definition at line 192 of file IxPerfProfAcc.h.
The documentation for this struct was generated from the following file: IxPerfProfAcc.h
Automatically generated from sources. © Intel Corp. 2003