Main Page Modules Alphabetical List Data Structures File List Data Fields Globals # IxHssAccPktHdlcFraming Struct Reference [IXP425 HSS Access (IxHssAcc) API] This structure contains information required by the NPE to configure the HDLC co-processor. More...
## Data Fields
IxHssAccPktHdlcIdleType | hdlcIdleType
| What to transmit when a HDLC port is idle.
IxHssAccBitEndian | dataEndian
| The HDLC data endianness.
IxHssAccPktCrcType | crcType
| The CRC type to be used for this HDLC port.
## Detailed Description This structure contains information required by the NPE to configure the HDLC co-processor. Definition at line 605 of file IxHssAcc.h. ## Field Documentation
IxHssAccPktCrcType IxHssAccPktHdlcFraming::crcType
| The CRC type to be used for this HDLC port. Definition at line 609 of file IxHssAcc.h.
IxHssAccBitEndian IxHssAccPktHdlcFraming::dataEndian
| The HDLC data endianness. Definition at line 608 of file IxHssAcc.h.
IxHssAccPktHdlcIdleType IxHssAccPktHdlcFraming::hdlcIdleType
| What to transmit when a HDLC port is idle. Definition at line 607 of file IxHssAcc.h.
The documentation for this struct was generated from the following file: IxHssAcc.h
Automatically generated from sources. © Intel Corp. 2003