Main Page Modules Alphabetical List Data Structures File List Data Fields Globals # IxAtmmVc Struct Reference [IXP425 ATM Manager (IxAtmm) API] This structure describes the required attributes of a virtual connection. More...
## Data Fields
unsigned | vpi
| VPI value of this virtual connection.
unsigned | vci
| VCI value of this virtual connection.
IxAtmmVcDirection | direction
| VC direction.
IxAtmTrafficDescriptor | trafficDesc
| Traffic descriptor of this virtual connection.
## Detailed Description This structure describes the required attributes of a virtual connection. Definition at line 166 of file IxAtmm.h. ## Field Documentation
IxAtmmVcDirection IxAtmmVc::direction
| VC direction. Definition at line 169 of file IxAtmm.h.
IxAtmTrafficDescriptor IxAtmmVc::trafficDesc
| Traffic descriptor of this virtual connection. This structure is defined by the IXP425 ATM Transmit Scheduler (IxAtmSch) API component. Definition at line 173 of file IxAtmm.h.
unsigned IxAtmmVc::vci
| VCI value of this virtual connection. Definition at line 168 of file IxAtmm.h.
unsigned IxAtmmVc::vpi
| VPI value of this virtual connection. Definition at line 167 of file IxAtmm.h.
The documentation for this struct was generated from the following file: IxAtmm.h
Automatically generated from sources. © Intel Corp. 2003