Main Page Modules Alphabetical List Data Structures File List Data Fields Globals # IxAtmdAccUtopiaConfig::UtTxTransTable2_ Struct Reference [IXP425 ATM Driver Access (IxAtmdAcc) Utopia Control API] Utopia Tx translation table Register. More...
## Data Fields
unsigned int | phy12:5
| [31-27] Tx Mapping value of logical phy 6
unsigned int | phy13:5
| [26-22] Tx Mapping value of logical phy 7
unsigned int | phy14:5
| [21-17] Tx Mapping value of logical phy 8
unsigned int | reserved_1:1
| [16-0] These bits are always 0
unsigned int | phy15:5
| [15-11] Tx Mapping value of logical phy 3
unsigned int | phy16:5
| [10-6] Tx Mapping value of logical phy 4
unsigned int | phy17:5
| [5-1] Tx Mapping value of logical phy 5
unsigned int | reserved_2:1
| [0] These bits are always 0
## Detailed Description Utopia Tx translation table Register. Definition at line 1185 of file IxAtmdAccCtrl.h. ## Field Documentation
unsigned int IxAtmdAccUtopiaConfig::UtTxTransTable2_::phy12
| [31-27] Tx Mapping value of logical phy 6 Definition at line 1188 of file IxAtmdAccCtrl.h.
unsigned int IxAtmdAccUtopiaConfig::UtTxTransTable2_::phy13
| [26-22] Tx Mapping value of logical phy 7 Definition at line 1190 of file IxAtmdAccCtrl.h.
unsigned int IxAtmdAccUtopiaConfig::UtTxTransTable2_::phy14
| [21-17] Tx Mapping value of logical phy 8 Definition at line 1192 of file IxAtmdAccCtrl.h.
unsigned int IxAtmdAccUtopiaConfig::UtTxTransTable2_::phy15
| [15-11] Tx Mapping value of logical phy 3 Definition at line 1196 of file IxAtmdAccCtrl.h.
unsigned int IxAtmdAccUtopiaConfig::UtTxTransTable2_::phy16
| [10-6] Tx Mapping value of logical phy 4 Definition at line 1198 of file IxAtmdAccCtrl.h.
unsigned int IxAtmdAccUtopiaConfig::UtTxTransTable2_::phy17
| [5-1] Tx Mapping value of logical phy 5 Definition at line 1200 of file IxAtmdAccCtrl.h.
unsigned int IxAtmdAccUtopiaConfig::UtTxTransTable2_::reserved_1
| [16-0] These bits are always 0 Definition at line 1194 of file IxAtmdAccCtrl.h.
unsigned int IxAtmdAccUtopiaConfig::UtTxTransTable2_::reserved_2
| [0] These bits are always 0 Definition at line 1202 of file IxAtmdAccCtrl.h.
The documentation for this struct was generated from the following file: IxAtmdAccCtrl.h
Automatically generated from sources. © Intel Corp. 2003